**CABRI 3000 CLOAKROOM LOCKERS**  
Doors:  
  
Made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float 10 mm, entire surface enamelled, all edges polished smooth. Colours according to standard colour range. Holes necessary for hinge and lock fixings drilled.  
  
Made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Listral SR200, 10 mm, (textured surface), entire surface enamelled, all edges polished smooth. Colours according to standard  
colour range. Holes necessary for hinge and lock fixings drilled.  
  
Floor and ceiling:  
  
Made of plastic, compressed, grey. Designed in such a way that a ventilation slot of locker width x 25 mm is created underneath. Upper ventilation with 45 x 6 mm slots. Floor with shoe rack, inclined at an angle of approx. 5% to allow water to run off.  
  
Partition walls and rear walls:  
  
Made of sheet aluminium, back bent with a radius of approx. 30 mm (easier to clean as no corners).  
  
Door hinges:  
  
Made of Al Mg Si alloy, mill finish, with maximum 90° opening. Stainless steel pin, nylon sliding surfaces, no lubrication, no corrosion.   
  
Door bumper and striking plate:  
  
Made of corrosion-resistant Al Mg Si alloy, mill finish, with firmly fixed plastic hollow profile as   
stop, not protruding, integrated into locker profile.  
  
Hat rack, coat hooks and clothes hanger hook:  
  
One clothes hanger hook per section, as well as a coat hook, both made of aluminium alloy,   
fastened to horizontally mounted, clear anodised tube. Hat rack consisting of two horizontally   
mounted tubes. There is no hat rack in half-size lockers and 3-storey lockers. Coat hook and double clothes hanger hook made of aluminium alloy.  
  
Anti-theft protection:  
  
Special lock frame with protruding lug that slots into the vertical locker profile. This prevents  
pressing the lock bolt open.  
  
Side wall cladding on lockers:  
  
Locker side walls that are visible are clad with a sheet of SR200, toughened unpolished glass, 10 mm thick, with coloured enamel on one side. The colour matches that of the door.

Locker heights 150, 170, 180, 195 cm  
Depth 50 cm  
Width 25, 30, 40 cm  
  
Base with trowelled surface finish provided by client.  
  
All lockers set up for ticket or coin-operated locks by Scheidt + Bachmann or Schulte-Schlagbaum (to be installed by customer).  
  
Construction parts:  
  
All connecting elements and the locker carcass are made of aluminium (DIN 1725), are 100%  
corrosion-resistant and environmentally friendly.  
100% recyclable.  
  
Enamelled safety glass:  
  
Enamels are lead- and cadmium-free, 100% recyclable.